(opts UsimANCA) (nil)
(opts UsimANCADepth) ""
(opts UsimANCADisplaySetting) (nil choices ("") value nil)
(opts UsimANCADv) "0.1"
(opts UsimANCAEnabled) nil
(opts UsimANCAExclude) ""
(opts UsimANCAInactive) "0"
(opts UsimANCANode) ""
(opts UsimANCAReportTitle) ""
(opts UsimANCATime) ""
(opts UsimDCA) (nil)
(opts UsimDCACheckType) "MOS Voltage"
(opts UsimDCACond) ""
(opts UsimDCADisplaySetting) (nil choices ("") value nil)
(opts UsimDCADurationTime) ""
(opts UsimDCAEnabled) nil
(opts UsimDCAInst) ""
(opts UsimDCAModel) ""
(opts UsimDCAPreserve) "No"
(opts UsimDCAProbe) "0"
(opts UsimDCAReportTitle) ""
(opts UsimDCASubckt) ""
(opts UsimDCATimeIntervals) ""
(opts UsimDCAVbcl) ""
(opts UsimDCAVbcu) ""
(opts UsimDCAVbel) ""
(opts UsimDCAVbeu) ""
(opts UsimDCAVbsl) ""
(opts UsimDCAVbsu) ""
(opts UsimDCAVcel) ""
(opts UsimDCAVceu) ""
(opts UsimDCAVcsl) ""
(opts UsimDCAVcsu) ""
(opts UsimDCAVdbl) ""
(opts UsimDCAVdbu) ""
(opts UsimDCAVdsl) ""
(opts UsimDCAVdsu) ""
(opts UsimDCAVesl) ""
(opts UsimDCAVesu) ""
(opts UsimDCAVgbl) ""
(opts UsimDCAVgbu) ""
(opts UsimDCAVgdl) ""
(opts UsimDCAVgdu) ""
(opts UsimDCAVgsl) ""
(opts UsimDCAVgsu) ""
(opts UsimDCAVpnl) ""
(opts UsimDCAVpnu) ""
(opts UsimDCAVsbl) ""
(opts UsimDCAVsbu) ""
(opts UsimNA) (nil)
(opts UsimNALimit) ""
(opts UsimNANodeNames) ""
(opts UsimNAOutputSort) "name"
(opts UsimNAReportTitle) ""
(opts UsimNASortIs) "inc"
(opts UsimNAStart) ""
(opts UsimNAStop) ""
(opts UsimOptMethod) nil
(opts UsimOptMethodHier) nil
(opts UsimPA) (nil)
(opts UsimPADepth) "1"
(opts UsimPADisplaySetting) (nil choices ("") value nil)
(opts UsimPAElemlen) "20"
(opts UsimPAEnabled) nil
(opts UsimPALimit) ""
(opts UsimPAName) ""
(opts UsimPAOutputSort) "avg"
(opts UsimPAPort) ""
(opts UsimPAPower) nil
(opts UsimPAReportTitle) ""
(opts UsimPATimeIntervals) ""
(opts UsimPCA) (nil)
(opts UsimPCACheckType) "Over Current"
(opts UsimPCADcpathCT) "50u"
(opts UsimPCADisplaySetting) (nil choices ("") value nil)
(opts UsimPCADurationTime) "5n"
(opts UsimPCAElements) ""
(opts UsimPCAEnabled) nil
(opts UsimPCAExiCT) "10u"
(opts UsimPCAFactor) ""
(opts UsimPCAFanout) "All Selected Nodes (0)"
(opts UsimPCAOvNodes) ""
(opts UsimPCAOvOption) "0"
(opts UsimPCAOvPreserve) "None"
(opts UsimPCAOvVmax) ""
(opts UsimPCAOvVmin) ""
(opts UsimPCAPSubckt) ""
(opts UsimPCAPreserve) "No"
(opts UsimPCAReportTitle) ""
(opts UsimPCASubcktChecked) ""
(opts UsimPCASubcktExcluded) ""
(opts UsimPCATimeChecked) "period"
(opts UsimPCATimeIntervals) ""
(opts UsimPCATimePoint) ""
(opts UsimPCAVSNodes) ""
(opts UsimPCAZNodes) ""
(opts UsimPCAZXSubckt) ""
(opts UsimPNA) (nil)
(opts UsimPNAElemThreshold) "10"
(opts UsimPNANode) (nil)
(opts UsimPRCSDisplaySetting) (nil choices ("") value nil)
(opts UsimPRCSEnabled) nil
(opts UsimPRCSFilePathName) ""
(opts UsimPRCSFileType) "SPF"
(opts UsimPRCSInstance) ""
(opts UsimRA) (nil)
(opts UsimRAAgeDomain) "loglog"
(opts UsimRAAgeMethod) "interp"
(opts UsimRAAgeproc) ""
(opts UsimRAAgingTime) "10y"
(opts UsimRADeltaD) 0.1
(opts UsimRADeltaDToggle) t
(opts UsimRAMinAge) 0.0
(opts UsimRAMode) "HCI only"
(opts UsimRANBTIAgeproc) ""
(opts UsimTA) (nil)
(opts UsimTACheckType) "setup"
(opts UsimTADepth) ""
(opts UsimTADisplaySetting) (nil choices ("") value nil)
(opts UsimTAEnabled) nil
(opts UsimTAMaxHighTime) ""
(opts UsimTAMaxLowTime) ""
(opts UsimTAMaxPerTime) ""
(opts UsimTAMinHighTime) ""
(opts UsimTAMinLowTime) ""
(opts UsimTAMinPerTime) ""
(opts UsimTANegWindow) ""
(opts UsimTARefSig) ""
(opts UsimTARefSigEdgeType) "rise"
(opts UsimTARefSigHighThreshold) ""
(opts UsimTARefSigLowThreshold) ""
(opts UsimTAReportTitle) ""
(opts UsimTASetupTime) ""
(opts UsimTASigEdgeType) "rise"
(opts UsimTASigHighThreshold) ""
(opts UsimTASigLowThreshold) ""
(opts UsimTASigNames) ""
(opts UsimTAStart) ""
(opts UsimTAStop) ""
(opts UsimTASubcktName) ""
(opts UsimTATrigger) "both"
(opts UsimUPS) (nil)
(opts UsimUPSDisplaySetting) (nil choices ("") value nil)
(opts UsimUPSpn) t
(opts UsimUPSpnAllWaveform) "Voltage for Tap Points"
(opts UsimUPSpnAuto) "Yes"
(opts UsimUPSpnAvgThreshold) ""
(opts UsimUPSpnFile) ""
(opts UsimUPSpnInst) ""
(opts UsimUPSpnIteration) "1"
(opts UsimUPSpnLevel) "Most Conservative (0)"
(opts UsimUPSpnMaxRes) ""
(opts UsimUPSpnMethod) "short"
(opts UsimUPSpnMethodOther) "short"
(opts UsimUPSpnModel) ""
(opts UsimUPSpnNode) ""
(opts UsimUPSpnOutputNode) ""
(opts UsimUPSpnPattern) ""
(opts UsimUPSpnPeakThreshold) ""
(opts UsimUPSpnRmsThreshold) ""
(opts UsimUPSpnSpeed) "Default (3)"
(opts UsimUPSpnWaveformFile) ""
(opts UsimVR) (nil)
(opts UsimVRName) ""
(opts UsimVRReportBox) (nil choices ("") value nil)
(opts UsimVRType) "Instance"
(opts abstoli) "1.00e-12"
(opts abstolv) "1.00e-06"
(opts analog) "Default (1)"
(opts cgnd) "1e-18"
(opts cgndr) "0"
(opts dc) "Complete DC (1)"
(opts dcut) nil
(opts dcut_field) ""
(opts diode_method) "Analog Table (A)"
(opts dump_step) ""
(opts elemcut_file) "0"
(opts emirEnable) nil
(opts emirStartTime) ""
(opts emirStopTime) ""
(opts lshort) "0"
(opts lvshort) "0"
(opts mos_cap) "Nonlinear (nl)"
(opts mos_method) "Analog/MS Table (A)"
(opts mt) "8"
(opts multithread) ""
(opts nodecut_file) "0"
(opts other) ""
(opts otherSpice) ""
(opts postl) "No RCR (0)"
(opts progress_p) ""
(opts progress_t) ""
(opts rcr_fmax) "1e9"
(opts rshort) "1.1e-3"
(opts rvshort) "1.1e-3"
(opts scale) "1.0"
(opts scalem) "1.0"
(opts simLoadFile) ""
(opts simRepeat) ""
(opts simRestart) nil
(opts simSave) nil
(opts simSaveFile) ""
(opts simTimePoints) ""
(opts sim_mode) "Mixed Signal (MS)"
(opts skip) nil
(opts skip_subckt) ""
(opts skip_subckt_insts) ""
(opts speed) "Default (5)"
(opts temp) "27"
(opts tnom) "27"
(opts tol) "0.01"
(opts wf_abstoli) "1e-12"
(opts wf_abstolv) "1e-6"
(opts wf_filter) t
(opts wf_reltol) ""
(opts wf_tres) "1e-12"
